Cross-Connection Control Program (CCCP) Review Sheet

Name of Waterworks: Click or tap here to enter text.
Classification of Waterworks: CWS ☐    NTNC ☐    TNC ☐
City/County: Click or tap here to enter text.
Ordinance: Yes ☐    No ☐    N/A ☐ 
PWSID#: Click or tap here to enter text.
Date CCCP Received: Click or tap to enter a date.
CCCP Date: Click or tap to enter a date.
Reviewed By: Click or tap here to enter text.
Program Type: Original ☐ 	Revised ☐ 	Previous Approval Date: Click or tap to enter a date.

1. Waterworks population: _______________________________________________________________
2. Number of Service Connections (Estimated)_______________________________________________
3. Source of water: Surface ☐ GUDI ☐ Well ☐ Spring ☐
4. Wholesale waterworks?  Yes ☐   No ☐
If yes, name of consecutive waterworks___________________________________________________
5. Consecutive waterworks?  Yes ☐   No ☐
If yes, name of wholesale waterworks____________________________________________________

CCCP Elements (Check ☐ all that applies)

	Program Element
	Yes
	No
	N/A

	All cross connection control program (CCCP) activities documented in a written plan. 12VAC5-590-580A 
	☐	☐	☐
	The plan addresses how the owner will ensure the cross-connections are adequately safeguarded. 12VAC5-590-580 B
	☐	☐	☐
	The plan addresses how the owner will address and approve the connection between auxiliary water systems and consumer’s water systems. 12VAC5-590-580 C
	☐	☐	☐
	The plan addresses maintaining acceptable working pressures (minimum 20 psig) in the distribution system to reduce the potential for backflow to occur. 12VAC5-590-580 D
	☐	☐	☐
	12VAC5-590-600. Cross-connection control program responsibilities.
	☐	☐	☐
	The owner shall review the CCCP and written cross-connection control plan not less than every five years and update it as necessary to satisfy the requirements of this chapter. The owner shall submit updates to the department to obtain approval. 12VAC5-590-600 A
	☐	☐	☐
	Plan identifies at least one individual assigned by the owner. 12VAC5-590-600 A
	☐	☐	☐
	CCCP not in conflict with the USBC and applicable building code regulations, including 13VAC5-63. 12VAC5-590-600 B
	☐	☐	☐
	CCCP shall ensure complete assessments of every consumer's water system and shall determine both the degree of hazard and the appropriateness of existing safeguards to prevent contamination from cross-connections and backflow. 12VAC5-590-600 C
	☐	☐	☐
	CCCP shall ensure testing, maintenance, and repairs of all backflow prevention assemblies, backflow elimination methods, and backflow prevention devices required and installed pursuant to 12VAC5-590-610. 12VAC5-590-600 D
	☐	☐	☐
	CCCP shall establish procedures for completing and monitoring operational tests, or other evaluation procedures as appropriate, at least annually, and after installation, relocation, or repairs, for testable backflow prevention assemblies, devices, and methods that provide containment. 12VAC5-590-600 E
	☐	☐	☐
	[Optional] CCCP includes a public education program includes the following minimum requirements:  
a. Causes of backflow; 
b. Hazards and health effects of cross-connections and backflow; 
c. Resources available to identify actual or potential cross-connections; 
d. Safeguards to use to eliminate or control the hazards at the point of use; and 
e. Sources for additional information. 12VAC5-590-600 E
	☐	☐	☐
	CCCP provides a method to discontinue or refuse water service to the consumer to ensure that the waterworks is adequately protected from cross-connections and backflow if any of the following conditions occur:
1. The consumer does not install, test and maintain a required backflow prevention assembly or backflow elimination method in accordance with the applicable sections of this chapter; 
2. The consumer allows a required backflow prevention assembly or backflow elimination method to become inoperable or the consumer removes or bypasses it; or 
3. The owner knows an unprotected or inadequately protected cross-connection exists on the premises and determines that there is inadequate backflow prevention at the service connection.  12VAC5-590-600 F
	☐	☐	☐
	In the event of backflow of contaminants into the waterworks, the owner shall promptly take or cause corrective action to confine and eliminate the contamination. The owner shall report the event to the department within one business day in the most expeditious manner. The owner shall submit a written report by the 10th day of the month following the month during which backflow occurred addressing the incident, its causes and effects, and safeguards required or other action taken. 12VAC5-590-600 G
	☐	☐	☐
	The owner shall maintain an inventory and records of testing, repairs, and maintenance of all backflow prevention assemblies, backflow elimination methods, and backflow prevention devices required and installed under 12VAC5-590-610 C. 12VAC5-590-600 H
	☐	☐	☐
	In the case of single-family residences subject to 12VAC5-590-610 C 5, the owner may determine whether or not to maintain an inventory or records. 12VAC5-590-600 H
	☐	☐	☐
	The owner shall maintain an inventory and records of testing, repairs, and maintenance of all backflow prevention assemblies, backflow elimination methods, and backflow prevention devices required and installed under 12VAC5-590-610 E. 12VAC5-590-600 I
	☐	☐	☐
	Maintain records related to the CCCP implementation, and any other records the department requires in accordance with 12VAC5-590-550 with a retention period of 10 years. 12VAC5-590-600 J
	☐	☐	☐
	12VAC5-590-610. Containment of backflow.
	
	
	

	Containment program consisting of backflow prevention assemblies or backflow elimination methods (i) at the service connection or (ii) downstream of the service connection but before any unprotected takeoffs 12VAC5-590-610 A
	☐	☐	☐
	Optional, in simple situations, point-of-use isolation protection by application of appropriate backflow prevention assemblies, backflow prevention devices, or backflow elimination methods complying with the USBC. 12VAC5-590-610 B
	☐	☐	☐
	A backflow prevention assembly or backflow elimination method shall be installed where the following conditions exist:
1. A substance is handled in such a manner as to create an actual or potential hazard to a waterworks (this shall include premises having sources or systems containing process fluids or waters originating from a waterworks which are no longer under the control of the owner); 
2. There exists internal cross-connections that, in the judgment of the owner or the department, may not be easily correctable or have intricate or complex plumbing arrangements that make it impracticable to determine whether or not cross-connections exist; 
3. There are security requirements or other prohibitions or restrictions that prevent the assessment of all potential cross-connections that may impair the quality of the water delivered; 
4. There is a repeated history of cross-connections being established or reestablished; 
5. There are fire protection systems, lawn sprinkler systems, or irrigation systems; 
6. The owner or department can show that a potential cross-connection hazard exists. 12VAC5-590-610 C
	☐	☐	☐
	Booster pumps or fire pumps connected to the waterworks shall be equipped with control devices to prevent a reduction of pump suction line pressure to less than 20 psig. 12VAC5-590-610 D
	☐	☐	☐
	A backflow prevention assembly or backflow elimination method shall be installed at consumer water systems serving the following types of facilities, including: 
1. Hospitals, mortuaries, clinics, veterinary establishments, nursing homes, and medical buildings; 
2. Laboratories; 
3. Piers, docks, and waterfront facilities; 
4. Sewage treatment plants, sewage pumping stations, or storm water pumping stations; 
5. Food and beverage processing plants; 
6. Chemical plants, dyeing plants, and pharmaceutical plants; 
7. Metal plating industries; 
8. Petroleum or natural-gas processing or storage plants; 
9. Radioactive materials processing plants or nuclear reactors; 
10. Car washes and laundries; 
11. Buildings with commercial, industrial, or institutional occupants served through a master meter; 
12. Water loading facilities; 
13. Slaughter houses and poultry processing plants; 
14. Farms where the water is used for other than household purposes; 
15. Commercial greenhouses and nurseries; 
16. Health clubs with swimming pools, therapeutic baths, hot tubs, or saunas; 
17. Paper and paper-product plants and printing plants; 
18. Pesticide or exterminating companies and their vehicles with storage or mixing tanks; 
19. Facilities that blend, store, package, transport, or treat chemicals, and their related vehicles; 
20. Schools or colleges with laboratory facilities; 
21. Highrise buildings (four or more stories); 
22. Multiuse commercial, office or warehouse facilities; and 
23. Others specified by the owner or the department when reasonable cause can be shown for a potential backflow or cross-connection hazard. 12VAC5-590-610 E
	☐	☐	☐
	All temporary or emergency service connections shall be protected where reasonable cause can be shown for a potential backflow or cross-connection hazard. Backflow prevention assemblies or backflow elimination methods used shall be appropriately certified or approved to match the requirements of this section. 12VAC5-590-610 F
	☐	☐	☐
	12VAC5-590-630. Backflow prevention assemblies, devices, and backflow elimination methods for containment.
	☐	☐	☐
	All backflow prevention assemblies or backflow elimination methods or backflow prevention devices shall be of the approved type and shall comply with the USBC. 12VAC5-590-630 A
	☐	☐	☐
	The backflow prevention assembly or backflow elimination method or backflow elimination device used shall depend on the degree of hazard that exists or may exist. 12VAC5-590-630 B 1
	☐	☐	☐
	The degree of hazard, either high or low 12VAC5-590-630 B 2
	☐	☐	☐
	The USBC and the manufacturer's specifications shall be used to determine the appropriateness of the backflow prevention assembly or backflow prevention device application for containment.  12VAC5-590-630  B 3
	☐	☐	☐
	Owners shall not allow the installation of backflow prevention devices or backflow prevention assemblies with openings, outlets, or vents that are designed to operate or open during backflow prevention: 
1. In areas subject to flooding or in pits; 
2. In areas with atmospheric conditions that represent a contamination threat to the potable water supply; and 
3. In such a manner as to be able to be bypassed. 12VAC5-590-630 C
	☐	☐	☐
	Starting January 1, 2023, persons testing and repairing backflow prevention assemblies and backflow prevention devices shall be certified by a Commonwealth of Virginia tradesman certification program (identified by DPOR as backflow prevention device workers). 12VAC5-590-630 D 
	☐	☐	☐


Plan Approval Recommended: Yes ☐    No ☐  

Comments:
__________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________
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